
**USB Driver Installation Instruction for (PLC) FC5A-D12**


**Installing on Windows XP**

**1.** Connect a USB cable to the USB port on the FC5A‐D12X1E (with power supplied) and the PC running.


**2.** After the message "Found New Hardware" appears on the PC, the driver installation wizard appears. Select **No, not this time** and click **Next**.



**3.** Select **Install the software automatically (Recommended)** and click **Next**.



**4.** Click **Continue Anyway** button.




If the installation is aborted without showing the dialog box above, **Block** is selected in the Driver Signing Options in **Driver Signing** in the **System Properties** dialog box. If the installation is aborted, this option should be changed to **Warn**. After changing the option to **Warn**, reconnect the Web server CPU module and retry the installation procedure from the step 1.

**5.** Installation is now complete. Click **Finish**.

**Installing on Windows Vista**


**1.** Connect a USB cable to the USB port on the FC5A‐D12X1E (with power supplied) and the PC running.

**2.** The dialog box below appears. Select **Locate and install driver software (recommended).**



**3.** The User Account Control dialog box appears. Click **Continue** button.

**4.** The dialog box below appears. Select **Install this driver software anyway**.




**5.** Installation is complete once the message “Your devices are ready to use” appears in the bottom right corner of the desktop.

**Installing on Windows 7 32‐bit or 64‐bit Edition**

**1.** Connect a USB cable to the USB port on the FC5A‐D12X1E (with power supplied) and the PC running.

**2.** The following message appears in the bottom right corner of the desktop.



**3.** Installation is complete once the message “Your device is ready to use” appears in the bottom right corner of the desktop.